W. Somkunthoda,e1, V. Amonkitbamrungb,e2, A. Charoenprakdeec,e3

and T. Seetawand,e4

*a* *Physics Department, Faculty of Science, Loei Rajabath University, Loei 42000, Thailand*

*b Department of Physics, Faculty of Science, Khon Kaen University, Khon Kaen, 41000, Thailand*

*c Hybrid Computing Research Laboratory, Faculty of Scienc Rajamugkara Technology Suvanaphum, Nontabureek, 10520, Thailand*

*d Thermoelectrics Research Center, Faculty of Science and Technology,*

*Sakon Nakhon Rajabhat University, Sakon Nakhon, 47000, Thailand*

[e1suphanchai@kbu.ac.th](mailto:e1suphanchai@kbu.ac.th), [e2vttaya@kku.ac.th](mailto:e2vttaya@kku.ac.th), [e3kmsomsak@kmitl.ac.th](mailto:e3kmsomsak@kmitl.ac.th), e4t\_seetawan@snru.ac.th

**Abstract**